Client: EMLab P&K (QA)
C/O: Mr. Quality Control
Re: Sample Report	Date of Sampling: 01-10-2013
Date of Receipt: 01-10-2013
Date of Report: 01-10-2013	

ASBESTOS AND OTHER FIBERS BY PCM: NIOSH 7400 METHOD

Location:	2:
Office	3:
Office	4:
Office	5:
Removal	6:
Removal	
Comments (see below)	None	None	None	None	None	
Lab ID-Version‡:	4534221-1	4534222-1	4534223-1	4534224-1	4534225-1	
Volume (liters)	900	900	900	150	150	
Fibers Detected	< 5.5	10	30.5	102	< 5.5	
Fields Read	100	100	100	20	100	
Fibers/mm²	< 7	12.74	38.85	649.68	< 7	
95% UCL*	< 0.003 (Sr = N/A)	0.009 (Sr = 0.13)	0.022 (Sr = 0.05)	2.059 (Sr = 0.09)	< 0.018 (Sr = N/A)	
Fibers per CC	< 0.003	0.005	0.017	1.668	< 0.018	

Comments: 

A counting rules used unless otherwise specified in report comments.
Interpretation is left to the company and/or persons who conducted the field work. 
Field blanks, if submitted with the project, have been used to correct the data.  Omission of 2 field blank samples should be considered a deviation from the NIOSH 7400 method.
Reporting limit is calculated using a minimum detection limit of 7 fibers/mm2.
* Upper 95% Confidence Limit for fibers/cc, calculated using a relative standard deviation value (intralaboratory Sr) mentioned above.
‡ A "Version" indicated by -"x" after the Lab ID# with a value greater than 1 indicates a sample with amended data.  The revision number is reflected by the value of "x".