Eurofins EPK Built Environment Testing, LLC
111 Anza Boulevard, Suite 122, Burlingame, CA 94010
(800) 651-4802  www.eurofinsus.com/Built

Client: EMLab P&K (QA)
C/O: Mr. Quality Control
Re: Sample Report	Date of Sampling: 01-11-2013
Date of Receipt: 01-11-2013
Date of Report: 01-11-2013	

SPORE TRAP REPORT: NON-VIABLE METHODOLOGY

Lab ID-Version‡
Location	Air vol. (L)	Background
Debris	Counts of Fungal
Structures	Fungal
Structures/m3	Presumptive Fungal ID
(raw counts*)	Percentage	
4537964-1
01/11/2013
1
Outside Reference

	75

	2+

	1
24
56
2
88
1
1
48
1
1
3
1

3
15	13  
320  
750  
27  
1,200  
13  
13  
640  
13  
13  
40  
13  
§ Total: 3,000  
40  
200  	Alternaria (1)
Ascospores (6)
Basidiospores (14)
Botrytis (2)
Cladosporium (22)
Epicoccum (1)
Fusarium (1)
Penicillium/Aspergillus types (12)
Pyricularia (1)
Rusts (1)
Smuts, Periconia, Myxomycetes (3)
Ulocladium (1)

Hyphal fragments (3)
Pollen (15)	< 1  
11  
25  
1  
39  
< 1  
< 1  
21  
< 1  
< 1  
1  
< 1  

N/A  
N/A  	
Comments: 	
4537965-1
01/11/2013
2

	75

	2+

	4
8
2
188
156
1
4

15
1	53  
110  
27  
2,500  
2,100  
13  
53  
§ Total: 4,800  
200  
13  	Ascospores (1)
Basidiospores (2)
Chaetomium (2)
Cladosporium (47)
Penicillium/Aspergillus types (39)
Smuts, Periconia, Myxomycetes (1)
Stachybotrys (4)

Hyphal fragments (15)
Pollen (1)	1  
2  
1  
52  
43  
< 1  
1  

N/A  
N/A  	
Comments: 	
4537966-1
01/11/2013
3

	75

	2+

	1
4
16
36
44
3

2	13  
53  
210  
480  
590  
40  
§ Total: 1,400  
27  	Alternaria (1)
Ascospores (1)
Basidiospores (4)
Cladosporium (9)
Penicillium/Aspergillus types (11)
Smuts, Periconia, Myxomycetes (3)

Hyphal fragments (2)	1  
4  
15  
35  
42  
3  

N/A  	
Comments: 	

Background debris indicates the amount of non-biological particulate matter present on the trace (dust in the air) and the resulting visibility for the analyst. It is rated from 1+ (low) to 4+ (high). Counts from areas with 4+ background debris should be regarded as minimal counts and may be higher than reported. It is important to account for samples volumes when evaluating dust levels.

The analytical sensitivity is the spores/m3 divided by the raw count. The limit of detection is the analytical sensitivity multiplied by the sample volume divided by 1000.

*All AIHA accredited laboratories are required to provide raw counts of fungal structures in spore trap reports. These counts are defined by AIHA as "Actual count without extrapolation or calculation". The number in parentheses next to the fungal type represents the exact number (or raw count) of fungal structures observed.

‡ A "Version" indicated by -"x" after the Lab ID# with a value greater than 1 indicates a sample with amended data.  The revision number is reflected by the value of "x".
§ Total has been rounded to two significant figures to reflect analytical precision.